*Український переклад нижче*

**Procurement notice**

**Ukraine**

**Project “Populations in Crisis: Access to Quality Healthcare”**

**(01.01.2024-31.12.2024)**

**Procurement of building materials / ASB/UKR/2023-11**

Arbeiter-Samariter-Bund e.V. (ASB) is a German non-government organization. ASB operates a Separate Subdivision in Ukraine in order to deliver humanitarian aid to the most vulnerable groups of the population affected by the conflict in Ukraine. In the framework of the project “Populations in Crisis: Access to Quality Healthcare” (01.01.2024-31.12.2024), funded by the «Nachbar in Not**»**, ASB Country Office Ukraine plans to purchase building materials.

Arbeiter-Samariter-Bund Deutschland e.V. now invites sealed bids from eligible bidders for:

**CONTRACT DESCRIPTION**

**Lot 1**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Name of product** | **Weight of item / size** | **Unit** | **Quantity**  **of items** | **Additional information** |
| 1 | Metal-plastic blind doors, interior | (width\*height)  900\*2000 cm | pc | 39 | Color: White. Handle-on the left (double-sided handle with lock (key-key)), open outwards open on yourself. Aluminum profile. No threshold. Horizontal jumper  Plastic filling (sandwich or thermal panel)  Number of cameras in the door-5  Number of cameras in a box-5  Door anchors-8-10 pieces (kit)  Door steel profile thickness - 1.5 mm  Window hinges. Knobs-push headset. The minimum color change period is 5 years |

**Lot 2**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Name of product** | **Weight of item / size** | **Unit** | **Quantity**  **of items** | **Additional information** |
| 1 | Ramp with wheelchair handrails | length 800 cm, width 120 cm. | pc | 1 | Solid metal construction –  Overhead ramp-portable with handrails, length when unfolded 800 cm, internal width 120 cm..  Handrail - 2 pcs.  Stainless steel handrails, outdoor ramp fence (handrails D 38 mm)  Rack height (upper edge)-100 cm.  Rack height (lower edge of the edge )-60 cm.  Detailed description:  Mounting the ramp to the wall from the right (right railing mounting on the wall without vertical posts)  Ramp tilt angle: no more than 8 degrees.  The height of the existing staircase is 60 cm.  Vertical handrail posts (material pipe steel diameter 38mm, thickness 2mm)  The distance between the posts is 100 cm.  Handrails: pipe steel 38mm diameter wall thickness 2.5 mm  Ramp floor material: "cutting" steel mesh thickness 3 mm  Floor frame span 35cm material: metal pipe 60 \* 40 thickness 2mm  Material type: steel |

**Lot 3**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Name of product** | **Weight of item / size** | **Unit** | **Quantity**  **of items** | **Additional information** |
| 1 | SHVVP wire | 3х2,5 | m.l. | 3000 |  |
| 2 | SHVVP wire | 2х1,5 | m.l. | 1274 |  |
| 3 | Linoleum for floors (commercial) | Width-3 m  Thickness-not less than 2.0 mm | m.sq. | 877 | Wear resistance class-34-medical institutions.  Abrasion group-T.  Color-brown, or light brown, gray or light gray.  All products are the same color. |
| 4 | Bimetallic radiators | Depth, mm: 120  Height, mm: 414  Center distance, mm: 350  Width, mm: 80  Number of Sections: 10 | pc | 39 | Maximum working pressure, bar: 46  Hydraulic test pressure, Bar: <52  Burst pressure, bar: >55  Maximum coolant temperature, °C: 110 |
| 5 | Ceramic floor tiles | 30 \* 30 cm. Thickness - from 8 mm. and thicker. | m.sq. | 120 | Tiles for Interior use. Square.  Matte, embossed. Porcelain stoneware.  Light gray, or gray in color . The drawing is monophonic. All products are the same color.  Abrasion class 5 / V |
| 6 | Ceramic wall tiles | 25 \* 40 cm. Thickness - from 6 mm. and thicker. | m.sq. | 283 | Tiles for Interior use.  Matte, or smooth. Porcelain stoneware.  Light cream, caramel or beige color. Drawing "under the stone", "under the marble", or with streaks. All products are the same color.  Abrasion class 5 / V |
| 7 | Alkyd enamel PF-266 | 2,8 kg | pc | 30 | Color: red-brown |
| 8 | Alkyd enamel | 2,8 kg | pc | 30 | Color: green |
| 9 | Alkyd enamel | 2,8 kg | pc | 30 | Color: white |
| 10 | Alkyd enamel | 2,8 kg | pc | 30 | Color: red |
| 11 | Acrylic facade paint (structural) | 10 l | pc | 300 | Color: white matte |
| 12 | Starting plaster | 25-30 kg or other | kg | 7080 | Base: gypsum; Type: Dry, starting; |
| 13 | Finishing putty | 25-30 kg or other | kg | 2000 | Base: gypsum; type: dry, finished |
| 14 | Primer | 10 l | pc | 40 | Deep penetration |
| 15 | Suspended ceiling "Armstrong" Assembly , including: |  | m.sq. | 800 |  |
| 1) | Suspended ceiling plate | 600х600х13 mm | pc | 1920 | Plate material-mineral fiber;  Drawing: white flat surface with a pattern of small perforations and small dots;  Surface Type-Matt; |
| 2) | Suspended ceiling profile start | 3600х20х22х0,25 mm | pc | 180 | Element of the metal structure of the suspended ceiling-wall corner L-shaped profile |
| 3) | Suspended ceiling profile 1.2 m | 1200х23х24х0,23 mm | pc | 1400 | Element of the metal structure of the suspended ceiling-transverse Guide T-shaped profile |
| 4) | Suspended ceiling profile 0,6 m | 600х23х24х0,23 mm | pc | 1410 | Element of the metal structure of the suspended ceiling-transverse Guide T-shaped profile |
| 5) | Suspended ceiling profile 3,6 m | 3600х23х32х0,25mm | pc | 165 | Element of the metal structure of the suspended ceiling – the main Guide T-shaped profile |

**Mandatory requirements for all materials**:

* quality certificates;
* shelf life at the time of delivery of goods shall not be less than 50% of the total shell life for each position;
* packaging must ensure full safety of the cargo during transportation in view of loading and unloading.

**Instruction to Tenderers**

1. ASB reserves the right to request samples to assess quality of items;
2. ASB reserves the right to increase or decrease the number of items and/or the quantity per item included in the order;
3. ASB reserves the right to place the order for items to different suppliers;
4. ASB reserves the right to place the order only for selected items;
5. the supplier shall provide a written warranty that the items are according to the above specifications and quality;
6. The offer must contain a complete list of products, otherwise the application will not be considered.
7. ASB reserves the right to decide not to award the contract and/or to cancel the tender procedure without providing explanations to participants.

**Delivery Point**

All items should be delivered to the warehouse as agreed with ASB in the Kiev region Vorzel city. The delivery and unload to the warehouse must be part of the total budget of the offer.

**Delivery Date**

When submitting bids, the tenderers should indicate the earliest possible date of delivery.

**Conditions for Participation in Tender:**

Bidders should meet the following criteria:

1. possess all necessary legal permissions or licenses required to carry out business activities in the country of operation;
2. have previous experience, knowledge and technical expertise to deliver the order;
3. provide financial and economic guarantees to deliver the order;
4. comply with the principles set forth in the Declaration for Candidates and Tenderers;
5. not fall under any of the exclusion criteria listed below.

**Grounds for exclusion from participation in contracts**

Candidates or tenderers will be excluded from participation in a procurement procedure if:

a) they are bankrupt or being wound up, are having their affairs administered by the courts, have entered into an arrangement with creditors, have suspended business activities, are the subject of proceedings concerning those matters, or are in any analogous situation arising from a similar procedure provided for in national legislation or regulations;

b) they have been convicted of an offence concerning their professional conduct by a

judgement which has the force of *res judicata*;

c) they have been guilty of grave professional misconduct proven by any means which the beneficiary of the grant can justify;

d) they have not fulfilled obligations relating to the payment of social security contributions or the payment of taxes in accordance with the legal provisions of the country in which they are established or with those of the country of the grant beneficiary or those of the country where the contract is to be performed;

e) they have been the subject of a judgement which has the force of *res judicata* for fraud, corruption, involvement in a criminal rganization or any other illegal activity detrimental to ASB financial interests;

f) following another procurement procedure or grant award procedure financed by ASB, they have been declared to be in serious breach of contract for failure to comply with their contractual obligations.

Candidates or tenderers must certify that they are not in one of the situations listed above.

**Exclusion from award of contracts**

Contracts may not be awarded to candidates or tenderers which, during the procurement procedure:

a) are subject to a conflict of interests;

b) are guilty of misrepresentation in supplying the information required by ASB as a condition of participation in the contract procedure or fail to supply this information.

**List of necessary documents for participation in the tender**

**Note**: *All blank spaces in the forms must be filled in. Erasing and corrections are not permitted*. *Where required, the documents should be duly signed and sealed by an authorized representative of the company. Pages that do not require a signature must be initialed and/or stamped.*

***For legal entities***:

1. Bid Submission Form;
2. Technical Specifications (accompanied by quality certificates);
3. Declaration for Candidates and Tenderers;
4. Price list
5. copies of pages of the Articles of Association: the first page, the page with the types of activities and the page about the powers of the director;
6. copies of the Certificate of State Registration (for registered before May 7, 2011, if they had no Extract) or an Extract from the Unified State Register of Legal Entities and Individual Entrepreneurs;
7. extract from the Unified State Register of Legal Entities and Individual Entrepreneurs, which indicates the main types of activities. The date of the extract formation should not exceed 2 months prior to the filing date;
8. certificate about the absence of arrears on taxes, fees, payments controlled by the state fiscal authorities (if certificate from fiscal authorities cannot be submitted before the deadline, please indicate the date when it can be submitted to ASB);
9. certificate about the absence of proceedings in bankruptcy case. Date of formation of the certificate should not exceed 21 days before the date of filing an application;
10. extract from the Register of tax payers of value added tax or single tax (if available);
11. licenses (if type of activity is licensed);
12. references confirming experience in performing similar projects.

***For Individual Entrepreneurs***:

1. Bid Submission Form;
2. Technical Specifications (accompanied by quality certificates);
3. Declaration for Candidates and Tenderers;
4. Price list;
5. copies of the Certificate of State Registration (for registered before May 7, 2011, if they had no Extract) or an Extract from the Unified State Register of Legal Entities and Individual Entrepreneurs;
6. extract from the Unified State Register of Legal Entities and Individual Entrepreneurs, which indicates the main types of activities;
7. certificate about the absence of arrears on taxes, fees, payments controlled by the state fiscal authorities (if certificate from fiscal authorities cannot be submitted before the deadline, please indicate the date when it can be submitted to ASB);
8. certificate about the absence of proceedings in bankruptcy case;
9. extract from the Register of tax payers of value added tax or single tax (if available);
10. licenses (if type of activity is licensed);
11. references confirming experience in performing similar projects.

**Submission Requirements**

1. All bids must be delivered in sealed envelopes;
2. The bid can be prepared in Ukrainian and/or English;
3. The bid offer MUST remain valid for a period of 60 days;
4. The bid documents MUST be arranged in the order indicated above;

The bids should be delivered to the following address:

Mailbox “**FOR TENDERS**” on the ground floor

Arbeiter-Samariter-Bund (ASB), Ukraine

18 Tadeusha Kostyushka St., Lviv 79000, Ukraine

**PROCEDURE**

Bidding will be conducted through the use of Arbeiter-Samariter-Bund Deutschland e.V.’s procurement guidelines which can be obtained from Arbeiter-Samariter-Bund Deutschland e.V. at Sülzburgstr. 140, 50937, Köln, Germany.

**SELECTION CRITERIA**

* сompliance with listed requirements
* high quality of items
* validity of the offer
* price
* terms of delivery
* terms of payment (%prepayment and % postpayment)
* previous experience in performing similar work
* Suppliers providing samples will get additional scores. The address for providing samples is 20b Antonovycha STR., Kiev. contact person is Vladimir Petrov directorasb@asb.org.ua

Arbeiter-Samariter-Bund Deutschland e.V. reserves the right to reject any offer if it does not meet the above requirements.

The bid process will be comprised of two stages. The first stage involves the evaluation of the bids with regard to formal requirements and completeness, while the second stage is the substantive evaluation according to the Selection Criteria defined by the Evaluation Committee.

The winning Tenderer will be chosen by ASB within 7 days. The Evaluation Committee will select the winning Tenderer after the conclusion of the negotiation sessions. The participants of tender will receive either selection or rejection letters.

**DEADLINE**

All bids must be delivered in sealed envelopes to the address below by the COB (**18.00) on 22 January 2024** and marked with the phrase: “**TENDER ASB/UKR/2023-11**”. Faxed/electronic bids will be rejected. Late bids will be rejected.

Mailbox “**FOR TENDERS**” on the ground floor

Arbeiter-Samariter-Bund (ASB), Ukraine

18 Tadeusha Kostyushka St., Lviv 79000, Ukraine

Please direct questions regarding the application process to the following e-mail address: [info@asb.org.ua](mailto:info@asb.org.ua). Please indicate the subject of the e-mail: “**Tender ASB/UKR/2023-11**”.The deadline for sending questions is **15 January 2024.**

**Повідомлення про закупівлю**

**Україна**

**Проект «Населення в кризовій ситуації: доступ до якісного медичного обслуговування»**

**(01.01.2024-31.12.2024)**

**Закупівля будівельних матеріалів / ASB/UKR/2023-11**

«Спілка робочих самаритян Німеччини з.С.» (ASB) – це німецька неурядова організація. ASB має відокремлений підрозділ в Україні, який надає гуманітарну допомогу найбільш вразливим групам населення, що постраждали внаслідок конфлікту в Україні. У рамках проекту «Населення в кризовій ситуації: доступ до якісного медичного обслуговування» (01.01.2024-31.12.2024), який фінансується «Nachbar in Not**»**, Відокремлений підрозділ ASB в Україні планує здійснити закупівлю будівельних матеріалів.

Спілка робочих самаритян Німеччини з.С. зараз приймає закриті конверти з тендерними пропозиціями від кандидатів, які відповідають критеріям, для:

**ОПИС КОНТРАКТУ**

**Лот 1**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Найменування продукту** | **Фасування / Розмір**  **(у кг/г/л)** | **Од.виміру** | **Кількість одиниць** | **Додаткова інформація** |
| 1 | Двері металопластикові глухі, міжкімнатні | (ширина\*висота)  900\*2000 см | шт. | 39 | Колір: Білий. Ручка – зліва (двухстороння ручка з замком (ключ-ключ)), відкриваються на себе  Алюмінієвий профіль. Без порогу. Горизонтальна перемичка. Заповнення пластик (сендвіч або термопанель)  Кількість камер в дверях-5  Кількість камер в коробці-5  Дверні анкерні пластини-8-10 штук (комплект)  Товщина сталевого профілю дверей- 1,5 мм  Петлі-віконні. Ручки -нажимний гарнітур. Мінімальний період зміни кольору-5 років |

**Лот 2**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Найменування продукту** | **Фасування / Розмір**  **(у кг/г/л)** | **Од.виміру** | **Кількість одиниць** | **Додаткова інформація** |
| 1 | Пандус з поручнями для інвалідних візків | довжина 800 см, ширина 120 см. | шт | 1 | Цільна металева конструкція –  Пандус накладний-переносний з поручнями, довжина в розкладеному стані 800 см, Внутрішня ширина 120 см..  Поручень -2 шт.  Поручні з нержавіючої сталі, огородження пандуса для вулиці (поручні D 38 мм)  Висота стійки (верхній край )-100 см.  Висота стійки (нижнього краю краю )-60 см.  Детальний опис:  Кріплення пандусу до стіни з права ( праве перило кріплення на стіну без вертикальних стійок)  Кут нахилу пандусу: не більше 8 градусів  Висота існуючих сходів 60 см  Вертикальні стійки поручнів (матеріал труба сталь діаметр 38мм, товщина 2мм)  Відстань між стійками 100 см.  Поручні: труба сталь 38мм діаметр товщина стінки 2,5мм  Матеріал підлоги пандуса: «просечка» стальна сітка товщина 3мм  Проліт каркасу підлоги 35см матеріал: труба металева 60\*40 товщина 2мм  Тип матеріалу: сталь |

**Лот 3**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Найменування продукту** | **Фасування / Розмір**  **(у кг/г/л)** | **Од.виміру** | **Кількість одиниць** | **Додаткова інформація** |
| 1 | Провід ШВВП | 3х2,5 | м.пог | 3000 |  |
| 2 | Провід ШВВП | 2х1,5 | м.пог. | 1274 |  |
| 3 | Лінолеум для підлоги (комерційний) | Ширина-3 м  Товщина- Не менше 2,0 мм | м.кв. | 877 | Клас зносостійкості-34 – медичні заклади.  Група стираності - Т.  Колір- Коричневи, або світлокоричневи, сірий або світло сірий.  Весь товар одного кольору. |
| 4 | Радіатори біметалічні | Глибина, мм: 120  Висота, мм: 414  Міжосьова відстань, мм: 350  Ширина, мм: 80  Кількість секцій: 10 | шт | 39 | Максимальний робочий тиск, бар: 46  Тиск при гідравлічних випробуваннях, бар: <52  Тиск на розрив, бар: >55  Максимальна температура теплоносія, °С: 110 |
| 5 | Плитка керамічна для підлоги | 30\*30 см. Товщина- від 8 мм. і товще. | м.кв. | 120 | Плитка для внутрішніх робіт. Квадратна.  Матова, рельєфна. Керамограніт.  Світлого сірого, або сірого кольору . Малюнок- однотонна. Весь товар одного кольору.  Клас стирання 5/V |
| 6 | Плитка керамічна для стін | 25\*40 см. Товщина- від 6 мм. і товще. | м.кв. | 283 | Плитка для внутрішніх робіт.  Матова, або гладка. Керамограніт.  Світлого кремового, карамельного або бежевого кольору. Малюнок «під камінь», «під мармур», або з розводами. Весь товар одного кольору.  Клас стирання 5/V |
| 7 | Емаль алкідна ПФ-266 | 2,8 кг | шт | 30 | Колір: червоно-коричнева |
| 8 | Емаль алкідна | 2,8 кг | шт | 30 | Колір: зелена |
| 9 | Емаль алкідна | 2,8 кг | шт | 30 | Колір: біла |
| 10 | Емаль алкідна | 2,8 кг | шт | 30 | Колір: червона |
| 11 | Фарба акрилова фасадна (структурна) | 10 л | шт | 300 | Колір: біла матова |
| 12 | Штукатурка стартова | 25-30 кг або інш. | кг | 7080 | Основа: гіпсова; тип: суха,стартова; |
| 13 | Шпаклівка фінішна | 25-30 кг або інш. | кг | 2000 | Основа: гіпсова; тип: суха,фінішна |
| 14 | Грунтовка | 10 л | шт | 40 | Глибокого проникнення |
| 15 | Стеля підвісна "Армстронг" в зборі ,  в тому числі: |  | м.кв | 800 |  |
| 1) | Плита підвісної стелі | 600х600х13мм | шт | 1920 | Матеріал плити – мінеральне волокно;  Малюнок: біла рівна поверхня з малюнком дрібної перфорації і невеликих крапок;  Тип поверхні – матовий; |
| 2) | Профіль підвісної стелі Старт | 3600х20х22х0,25мм | шт | 180 | Елемент металоконструкції підвісної стелі – пристінний куток L-подібний профіль |
| 3) | Профіль підвісної стелі 1,2м | 1200х23х24х0,23мм | Шт | 1400 | Елемент металоконструкції підвісної стелі – поперечний направляючий Т-подібний профіль |
| 4) | Профіль підвісної стелі 0,6м | 600х23х24х0,23мм | шт | 1410 | Елемент металоконструкції підвісної стелі – поперечний направляючий Т-подібний профіль |
| 5) | Профіль підвісної стелі 3,6м | 3600х23х32х0,25мм | шт | 165 | Елемент металоконструкції підвісної стелі – основний направляючий Т-подібний профіль |

**Обов’язкова вимога до всіх матеріалів**:

* сертифікати якості;
* термін придатності на момент доставки товарів має бути не меншим, ніж 50% загального терміну придатності для кожного найменування;
* упаковка повинна забезпечувати повну безпеку вантажу під час перевезення з урахуванням завантаження і розвантаження.

**Інструкція для учасників тендеру**

1. ASB залишає за собою право затребувати зразки для оцінки якості продуктів;
2. ASB залишає за собою право збільшувати або зменшувати кількість одиниць предметів та/або предмету, що входить до замовлення;
3. ASB залишає за собою право замовляти товари у різних постачальників;
4. ASB залишає за собою право замовляти лише обрані товари;
5. постачальник повинен надати письмову гарантію, що товари відповідають вищевказаним характеристикам та стандартам якості;
6. Пропозиція повинна містити повний перелік товарів, інакше заявка не розглядатиметься.
7. ASB залишає за собою право вирішити не підписувати договір та/або відмінити тендер без надання пояснень учасникам.

**Місце доставки**

Всі товари слід доставити на склад за домовленістю із ASB у Київській області м.Ворзель. Доставка та розвантаження на склад повинна бути частиною загального бюджету пропозиції.

**Дата доставки**

Подаючи заявки, учасники тендеру повинні зазначити найранішу дату можливої доставки.

**Умови участі у тендері:**

Учасники тендеру повинні відповідати наступним критеріям:

1. володіти всіма необхідними юридичними дозволами чи ліцензіями для здійснення підприємницької діяльності у країні здійснення діяльності;
2. мати попередній досвід, знання та технічну експертизу для виконання замовлення;
3. надати фінансові та економічні гарантії виконання замовлення;
4. дотримуватись положень, викладених у декларації для кандидатів та учасників тендерів;
5. не підпадати під жоден із перерахованих нижче критеріїв виключення.

**Підстави для виключення з участі у торгах**

Кандидати чи учасники тендеру будуть виключені з участі у процедурі закупівлі, якщо:

1. вони банкрутують або закриваються, ведуть справи у судах, уклали угоду з кредиторами, призупинили підприємницьку діяльність, підлягають провадженню у цих справах або знаходяться у будь-якій аналогічній ситуації, що виникає внаслідок подібної процедури, передбаченої національним законодавством чи нормативними актами;
2. їх засудили за правопорушення, що стосується їхньої професійної поведінки,  
   рішенням, яке має силу *res judicata*;
3. вони винні у тяжких посадових порушеннях, що доведено у будь-який спосіб, який бенефіціар гранту може обґрунтувати;
4. вони не виконали зобов’язань щодо сплати внеску на соціальне страхування або сплати податків відповідно до законодавчих норм країни, в якій вони зареєстровані, або країни бенефіціара гранту, або країни, де договір має бути виконаний;
5. щодо них було прийняте судове рішення, яке має силу *res judicata*, за шахрайство, корупцію, причетність до злочинної організації або будь-яку іншу незаконну діяльність, що може завдати шкоди фінансовим інтересам ASB;
6. після іншої процедури закупівлі або процедури надання гранту, що фінансувалися ASB, вони були оголошені серйозними порушниками договору за невиконання своїх договірних зобов’язань.

Кандидати чи учасники тендеру повинні підтвердити, що вони не перебувають в одній із перелічених вище ситуацій.

**Винятки з укладення договорів**

Договори не можуть бути укладені з кандидатами або учасниками тендеру, які під час процедури закупівлі:

а) підлягають конфлікту інтересів;

б) винні у наданні недостовірної інформації або не наданні інформації, яка вимагається ASB як умова участі у договірній процедурі.

**Перелік документів, необхідних для участі у тендері**

**Увага**: *Усі порожні місця у формах повинні бути заповнені. Стирання та виправлення не дозволяються. Документи повинні бути належним чином підписані та затверджені печаткою уповноваженого представника компанії відповідно до вимог. Сторінки, які не потребують підпису, повинні бути засвідчені ініціалами та/або скріплені печаткою.*

***Для юридичних осіб****:*

1. заявка з тендерною пропозицією;
2. технічні специфікації (що супроводжуються сертифікатами якості);
3. декларація для кандидатів та учасників тендерів;
4. каталог цін;
5. копії сторінок Статуту організації – першої сторінки, сторінки з видами діяльності та сторінки про повноваження директора;
6. копії свідоцтва про державну реєстрацію (для зареєстрованих до 07.05.2011 року, якщо вони не отримали витяг) або витяг з Єдиного державного реєстру юридичних осіб та фізичних осіб-підприємців;
7. витяг з Єдиного державного реєстру юридичних осіб та фізичних осіб-підприємців, в якому зазначаються основні види діяльності. Дата формування витягу не повинна перевищувати 2 місяці до дати подання заявки;
8. довідка про відсутність заборгованості по податках, зборах, платежах, що контролюються державними фіскальними органами (якщо довідка від фіскальних органів не може бути подана до кінцевого терміну, вкажіть будь ласка, дату, коли вона може бути подана ASB);
9. довідка про відсутність провадження у справі про банкрутство. Дата формування довідки не повинна перевищувати 21 день до дати подання заявки;
10. витяг з реєстру платників податку на додану вартість або єдиного податку (за наявності);
11. ліцензії (якщо вид діяльності ліцензується);
12. довідки, що підтверджують досвід виконання подібних проектів.

***Для фізичних осіб-підприємців (ФОП)****:*

1. заявка з тендерною пропозицією;
2. технічні специфікації (що супроводжуються сертифікатами якості);
3. декларація для кандидатів та учасників тендерів;
4. каталог цін
5. копії свідоцтва про державну реєстрацію (для зареєстрованих до 07.05.2011 року, якщо вони не отримали витяг) або витяг з Єдиного державного реєстру юридичних осіб та фізичних осіб-підприємців;
6. витяг з Єдиного державного реєстру юридичних осіб та фізичних осіб-підприємців, в якому зазначаються основні види діяльності;
7. довідка про відсутність заборгованості по податках, зборах, платежах, що контролюються державними фіскальними органами (якщо довідка від фіскальних органів не може бути подана до кінцевого терміну, вкажіть будь ласка, дату, коли вона може бути подана ASB);
8. довідка про відсутність провадження у справі про банкрутство;
9. витяг з реєстру платників податку на додану вартість або єдиного податку (за наявності);
10. ліцензії (якщо вид діяльності ліцензується);
11. довідки, що підтверджують досвід виконання подібних проектів.

**Вимоги до подання**

a) усі тендерні пропозиції повинні бути доставлені у заклеєних конвертах;

б) тендерна пропозиція може бути подана українською і/або англійською мовою;

в) тендерна пропозиція ПОВИННА залишатися дійсною протягом 60 днів;

г) тендерні документи ОБОВ’ЯЗКОВО мають бути складені у тому порядку, як зазначено вище;

д) заявки повинні бути доставлені за наступною адресою:

Поштова скринька “**FOR TENDERS**” на першому поверсі

Спілка робітничих самаритян (ASB), Україна

м .Львів 79000, Україна

вул. Т.Костюшко 18

**ПРОЦЕДУРА**

Тендер буде проведений згідно з правилами закупівель Спілки робітничих самаритян Німеччини з.С., які можна отримати у Спілці робітничих самаритян Німеччини з.С. на Зюльцбурґштрасе 140, 50937, м. Кельн, Німеччина.

**КРИТЕРІЇ ВІДБОРУ**:

* відповідність зазначеним вимогам
* висока якість товарів
* термін дії пропозиції
* ціна
* умови доставки
* умови оплати (% передоплати та % післяплати)
* попередній досвід виконання подібної роботи
* Постачальники, які надають зразки, отримають додаткові бали. Адреса для надання зразків – м.Київ, вул. Антоновича 20б, офіс 24; Контактна особа: Володимир Петров, directorasb@asb.org.ua

Спілка робітничих самаритян Німеччини з.С. залишає за собою право відхиляти пропозиції, якщо вони не відповідають зазначеним вище вимогам.

Процедура торгів буде складатися з двох етапів. Під час першого етапу пропозиції оцінюються з огляду на дотримання формальних вимог та повноту, а другий етап - це змістова оцінка відповідно до критеріїв відбору, визначених Комітетом з оцінки тендерних пропозицій.

Переможець тендеру буде обраний ASB протягом 7 днів. Комітет з оцінки тендерних пропозицій обере переможця тендеру після завершення переговорних сесій. Учасники тендеру отримають листи про відбір або відмову.

**КІНЦЕВИЙ ТЕРМІН ПОДАННЯ ЗАЯВ**

Усі тендерні пропозиції повинні бути доставлені у заклеєних конвертах, позначених написом “**TENDER ASB/UKR/2023-11**”, до кінця робочого дня (18.00) **22 січня 2024 року** за вказаною нижче адресою. Тендерні пропозиції, надіслані факсом або електронною поштою, будуть відхилені. Пропозиції, які надійдуть після дедлайну, будуть відхилені.

Поштова скринька “**FOR TENDERS**” на першому поверсі

Спілка робочих самаритян Німеччини

м .Львів 79000, Україна

вул. Т.Костюшко 18

Просимо надсилати запитання щодо процесу подання заявки на наступну електронну адресу: [info@asb.org.ua](mailto:info@asb.org.ua). В темі листа необхідно вказати: «**Тендер ASB/UKR/2023-11**».Останній день для надсилання запитань: **15 січня 2024 року.**